{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["服务报价"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"服务报价","index":0,"n_rows":10,"n_cols":13,"rows_kept":10,"merged":[[1,0,1,12],[2,6,2,7],[3,6,3,7],[5,6,5,7],[7,9,7,10],[8,9,8,10],[9,9,9,10]],"flags":["formulas_cached_only"]}
["附件"]
["广州市番安驾驶学校有限公司采购番禺区交警七中队无人机项目场地改造工程项目报价单"]
["序号","服务名称","公司（品牌）名称","规格","单位","数量","单价（元）",null,"总价（元）","提供服务内容","价格说明","服务保障说明","备注"]
["例子","广州市番安驾驶学校有限公司采购番禺区交警七中队无人机项目场地改造工程项目",null,"项","项",1,{"$nulls":3},"（1）造星瓦围墙围蔽，围墙总长116米，2米高，要求：用0.426彩色单瓦，40*40*2.0mm镀锌方管为柱，25*38*1.5mm扁管为副横，3米一柱，6米一顶，造柱顶基础。\n（2）造铁门，规格：5.4米长，2米高；共2扇。\n（3）地面平整，面积1296㎡，用钩机钩平地面，压实，地面铺6cm厚沥青渣，压平。\n（4）小课室翻新：室内室外扇灰，面积约185㎡。更换室内石膏天花，面积约61㎡。翻新铁门两套。地面扫油漆，面积约61㎡。屋顶星瓦补漏。\n（5）造休息棚，规格：3米*6米*2.8米，要求：柱用80*80*3.0cm方管镀锌，副横用75*45*2.0cm扁管，顶盖双面夹瓦，3面墙用隔墙板，正面用铝合金隔墙玻璃带门，底用15厘厚夹板。\n（6）清理小课室室内外垃圾、杂物和杂草。\n（7）修剪场内部分树木。",null,null,"报价时请将此行删除"]
[1]
["合计"]
[]
[{"$nulls":9},"报价单位（盖章）："]
[{"$nulls":9},"联系人和联系电话："]
[{"$nulls":9},"报价日期："]